---
title: Configure hardware Connector · Cloudflare Magic WAN docs
description: In this page you will find instructions on how to configure Magic
  WAN Connector. This guide provides a step-by-step guide for Magic WAN
  Connector initial setup. You can either return here after setting up your
  Magic WAN Connector, or refer to the Maintenance section where you will find
  instructions on how to update your settings.
lastUpdated: 2025-11-04T17:07:51.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/
  md: https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/index.md
---

In this page you will find instructions on how to configure Magic WAN Connector. This guide provides a step-by-step guide for Magic WAN Connector initial setup. You can either return here after setting up your Magic WAN Connector, or refer to the [Maintenance](https://developers.cloudflare.com/magic-wan/configuration/connector/maintenance/) section where you will find instructions on how to update your settings.

## Prerequisites

You need to purchase [Magic WAN](https://www.cloudflare.com/magic-wan) before you can purchase and use Magic WAN Connector. Magic WAN Connector can function as your primary edge device for your network, or be deployed in-line with existing network gear.

You also need to purchase Magic WAN Connector before you can start configuring your settings in the Cloudflare dashboard. Contact your account representative to learn more about purchasing options for Magic WAN Connector.

***

## Before you begin

There are a couple of decisions you need to make when installing your Magic WAN Connector. Refer to the topics below for more information.

### Determine the need for a high availability configuration

You can install up to two instances of Magic WAN Connector for redundancy at each of your sites. If one of your devices fails, traffic will fail over to the other, ensuring that you never lose connectivity to that site.

In this type of high availability (HA) configuration, you will choose a reliable LAN interface as the HA link which will be used to monitor the health of the peer connector. HA links can be dedicated links or can be shared with other LAN traffic.

You must decide the type of configuration you want for your site from the beginning: no redundancy or with redundancy. You cannot add redundancy after finishing the configuration of your dashboard settings. If, at a later stage, you decide to enable redundancy, you will need to delete your Magic WAN Connector device in the Cloudflare dashboard, and start again.

Do you need a high availability configuration?

* If you need a high availability configuration for your premises, refer to [About high availability configurations](#about-high-availability-configurations) for more information and learn how to configure your Magic WAN Connector device in this mode.

* If you do not need a high availability configuration for you premises, check if you need a [DHCP or a static IP setup](#decide-on-dhcp-vs-static-ip-connections) before proceeding to [Set up Cloudflare dashboard](#set-up-cloudflare-dashboard).

Warning

You cannot enable high availability for an existing Magic WAN Connector on-ramp. To add high availability to an existing Magic WAN Connector on-ramp in the Cloudflare dashboard, you need to delete the on-ramp and start again. Plan accordingly to create a high availability configuration from the start if needed.

### Decide on DHCP vs static IP connections

You can use Magic WAN Connector in both DHCP networks and networks that require a static IP configuration. At first boot, however, Magic WAN Connector needs to reach out to Cloudflare to download your settings and go through the activation process. If any of the networks plugged into your Magic WAN Connector device are DHCP enabled, do not use a VLAN, and have an Internet connection, that process is handled automatically. However, if all of the networks require more information to utilize, (such as a network with static IPs, or tagged VLAN networks) your Magic WAN Connector might need some more information to proceed.

There are couple of ways to provide this information. Choose the one that fits your workflow:

#### Option one - Activate on a DHCP Network

1. Connect Magic WAN Connector to a DHCP port with access to the Internet.
2. Go through the [setup flow](#set-up-cloudflare-dashboard) below and activate your Magic WAN Connector device.
3. Refer to [WAN with a static IP address](#wan-with-a-static-ip-address).

#### Option two - Bootstrap via Serial Console

Refer to the [Bootstrap workflow](#bootstrap-via-serial-console).

***

## Port speeds

The hardware version of the Magic WAN Connector includes two [SFP+ ports](https://en.wikipedia.org/wiki/Small_Form-factor_Pluggable) that support 10G throughput, as well as six RJ45 ports that support 1G throughput.

Refer to [](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/sfp-port-information)SFP+ port information for details on this topic.

***

## Set up Cloudflare dashboard

### Register your Connector

To set up and use the hardware version of Magic WAN Connector, you first need to register it with your account. This is not applicable to Virtual Magic WAN Connector.

1. In the Cloudflare dashboard, go to Magic WAN's **Configuration** page.[ Go to **Configuration**](https://dash.cloudflare.com/?to=/:account/magic-wan/configuration)
2. Under **Connectors**, select **Register your appliance**.

1) In **Appliance details** > **Serial number**, insert the serial number for your device. You can optionally add notes about the Magic WAN Connector you are adding to the dashboard.
2) (Optional) Select **Add** below **Serial number** to add multiple Magic WAN Connectors at once to your account.
3) Select **Register appliance**.

Your device is now registered with your account.

### Add a Connector on-ramp

You need to add your Magic WAN Connector to your Cloudflare dashboard and configure its settings before connecting it to the Internet.

To add a Magic WAN Connector:

1. Log in to the [Cloudflare dashboard](https://dash.cloudflare.com/) and select your account.
2. Go to **Magic WAN** > **Connector on-ramps (beta)**.
3. Select **Add**.

1) In **Name**, enter a descriptive name for your Magic WAN Connector. Optionally, you can also add a description for it.
2) You need to decide if you want to turn on high availability for the Magic WAN Connector. Refer to [About high availability configurations](#about-high-availability-configurations) for more information.
3) Select **Create and continue**.
4) Select **Add Connector**. This will show you a list of devices associated with your account. You need to have bought a Connector already for it to show up here. Refer to [Prerequisites](#prerequisites) if no Connector shows up in this list.
5) If you have more than one Magic WAN Connector, choose the one that corresponds to the on-ramp you are creating. Magic WAN Connector devices are identified by a serial number, also known as a service tag. Use this information to choose the right Magic WAN Connector.\
   Select **Add Connector** when you are ready to proceed.
6) Magic WAN Connector will be added to your account with an **Interrupt window** defined. The interrupt window is the time period when the Magic WAN Connector software can update, which may result in interruption to existing connections. You can change this later. Refer to [Interrupt window](https://developers.cloudflare.com/magic-wan/configuration/connector/maintenance/interrupt-service-window/) for more details on how to define when the Magic WAN Connector can update its systems.
7) Select **Continue** to proceed to creating your WAN and LAN networks.

### Create a WAN

* Dashboard

  When you have more than one anycast IP configured in your account (set up during your Magic WAN onboarding), Magic WAN Connector will automatically create at most two tunnels per WAN port. This improves reliability and performance, and requires no additional configuration on your part.

  1. In **WAN configuration**, select **Create**. You can create one or more [wide area networks (WANs)](https://www.cloudflare.com/learning/network-layer/what-is-a-wan/). Configuring multiple WANs will create multiple IPsec tunnels (one IPsec tunnel per WAN port). This allows Magic WAN Connector to load balance traffic over WANs of equal priority. It also allows Magic WAN Connector to failover between circuits according to their [health](https://developers.cloudflare.com/magic-wan/reference/tunnel-health-checks/). Refer to [WAN settings](https://developers.cloudflare.com/magic-wan/configuration/connector/reference/#wan-settings) for more details.

     Note

     This is not the same as a high availability (HA) configuration. HA configurations need two Magic WAN Connector devices to work. Refer to [About high availability configurations](#about-high-availability-configurations) for more information.

  2. In **Interface name**, enter a descriptive name for your WAN.

  3. **Interface number** refers to the physical Magic WAN Connector Ethernet port that you are using for your WAN. The ports are labeled `GE1`, `GE2`, `GE3`, `GE4`, `GE5`, and `GE6`. Choose the number corresponding to the port that you are using in Connector.\
     If you need a throughput higher than 1 Gbps, you can use one of the SFP+ ports. Refer to [SFP+ port information](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/sfp-port-information/) for more information on the hardware supported.

  4. In **VLAN ID**, enter a number between `0` and `4094` to specify a [VLAN ID](https://developers.cloudflare.com/magic-wan/configuration/connector/reference/#vlan-id).

  5. In **Priority**, choose the priority for your WAN. Lower numbers have higher priority. Refer to [Traffic steering](https://developers.cloudflare.com/magic-wan/reference/traffic-steering/) to learn more about how Cloudflare calculates priorities.

  6. In **Health check rate** configure the health check frequency for your site. Options are `low`, `mid`, and `high`. Refer to [Update tunnel health checks frequency](https://developers.cloudflare.com/magic-wan/configuration/common-settings/update-tunnel-health-checks-frequency/) for more information.

  7. **Addressing**: Select **DHCP**. This is needed the first time you set up your Magic WAN Connector to successfully download all settings to the machine and activate it. If you need a static IP address in your network environment:

     1. Continue the set up flow below to activate your Magic WAN Connector.
     2. Refer to [WAN with a static IP address](#wan-with-a-static-ip-address). If you choose a static IP, you also need to specify the static IP and gateway addresses.

  8. Select **Save** when you are finished.

* API

  Note

  You will need your [account ID](https://developers.cloudflare.com/fundamentals/account/find-account-and-zone-ids/) and [API token](https://developers.cloudflare.com/fundamentals/api/get-started/account-owned-tokens/) to use the API.

  Make a `POST` request [using the API](https://developers.cloudflare.com/api/resources/magic_transit/subresources/sites/subresources/wans/methods/create/) to create a WAN.

  The `static_addressing` object is optional. Omit it if you are using DHCP. If you are using static addressing, add the `secondary_address` parameter when your site is in high availability (HA) mode.

  Example:

  ```bash
  curl https://api.cloudflare.com/client/v4/accounts/{account_id}/magic/sites/{site_id}/wans \
  --header "X-Auth-Email: <EMAIL>" \
  --header "X-Auth-Key: <API_KEY>" \
  --header "Content-Type: application/json" \
  --data '{
    "name": "<YOUR_WAN_NAME>",
    "physport": 1,
    "priority": 0,
    "vlan_tag": 0
  }'
  ```

### Create a LAN

* Dashboard

  1. In **LAN configuration**, select **Create**.

  2. Enter a descriptive name for your LAN in **Interface name**.

  3. **Interface number** refers to the physical Magic WAN Connector Ethernet port that you are using for your WAN. The ports are labeled `GE1`, `GE2`, `GE3`, `GE4`, `GE5`, and `GE6`. Choose a number corresponding to the port that you are using in Connector.\
     If you need a throughput higher than 1 Gbps, you can use one of the SFP+ ports. Refer to [SFP+ port information](https://developers.cloudflare.com/magic-wan/configuration/connector/configure-hardware-connector/sfp-port-information/) for more information on the hardware supported.

  4. In **VLAN ID**, specify a [VLAN ID](https://developers.cloudflare.com/magic-wan/configuration/connector/reference/#vlan-id) to create virtual LANs.

  5. In **Static addressing** > **Static address** give your Magic WAN Connector's LAN interface its IP address. You can also enable the following options if they suit your use case:

     * **This is a DHCP server**: If your Magic WAN Connector is a [DHCP server](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/dhcp/dhcp-server/).
     * **This is a DHCP relay**: If your Magic WAN Connector is a [DHCP relay](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/dhcp/dhcp-relay/).

  6. (Optional) In **Directly attached subnet** > **Static NAT prefix**, enter a CIDR prefix to enable NAT (network address translation). The prefix you enter here should be the same size as the prefix entered in **Static addressing**. For example, both networks have a subnet mask of `/24`: `192.168.100.0/24` and `10.10.100.0/24`.

  7. (Optional) If your LAN contains additional subnets behind a layer 3 router, select **Add routed subnet** under **Routed subnets** to add them:

     * **Prefix**: The CIDR prefix for the subnet behind the L3 router.
     * **Next hop**: The address of the L3 router to which the Magic WAN Connector should forward packets for this subnet.
     * **Static NAT prefix**: Optional setting. If you want to enable NAT for a routed subnet, supply an "external" prefix for the overlay-facing side of the NAT to use. It must be the same size as **Prefix**.\
       Refer to [Routed subnets](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/routed-subnets/) for more information.

  8. Select **Save**.

  9. Select **Done** to finish your configuration. Tunnels and static routes will be automatically created for your Magic WAN Connector, once it boots up.

* API

  Note

  You will need your [account ID](https://developers.cloudflare.com/fundamentals/account/find-account-and-zone-ids/) and [API token](https://developers.cloudflare.com/fundamentals/api/get-started/account-owned-tokens/) to use the API.

  Make a `POST` request [using the API](https://developers.cloudflare.com/api/resources/magic_transit/subresources/sites/subresources/lans/methods/create/) to create a LAN.

  Example:

  ```bash
  curl https://api.cloudflare.com/client/v4/accounts/{account_id}/magic/sites/{site_id}/lans \
  --header "X-Auth-Email: <EMAIL>" \
  --header "X-Auth-Key: <API_KEY>" \
  --header "Content-Type: application/json" \
  --data '{
    "name": "<YOUR_LAN_NAME>",
    "physport": 2,
    "static_addressing": {
      "address": "172.16.14.0/24"
    },
    "vlan_tag": 0
  }'
  ```

#### Network segmentation

After setting up your LANs, you can configure your Magic WAN Connector to enable communication between them without traffic leaving your premises. Refer to [Network segmentation](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/network-segmentation/) for more information.

#### DHCP options

Magic WAN Connector supports different types of DHCP configurations. Magic WAN Connector can:

* Connect to a DHCP server or use a static IP address instead of connecting to a DHCP server.
* Act as a [DHCP server](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/dhcp/dhcp-server/).
* Use [DHCP relay](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/dhcp/dhcp-relay/) to connect to a DHCP server outside the location your Magic WAN Connector is in.
* [Reserve IP addresses](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/dhcp/dhcp-static-address-reservation/) for specific devices on your network.

### Add your Magic WAN Connector to a site

After finishing your Magic WAN Connector configuration, you need to add it to a site.

Sites represent the local network of a data center, office, or other physical location, and combine all on-ramps available there. Sites also allow you to check, at a glance, the state of your on-ramps and set up health alert settings so that you get notified when there are issues with the site's on-ramps.

Refer to [Set up a site](https://developers.cloudflare.com/magic-wan/configuration/common-settings/sites/) for more information.

## Set up your Magic WAN Connector

### Device installation

There are several deployment options for Magic WAN Connector. Magic WAN Connector can act like a DHCP server for your local network, or integrate with your local setup and have static IP addresses assigned to it.

When Magic WAN Connector acts like the WAN router for your site, deployment will be something like this:

```mermaid
flowchart LR
	accTitle: Magic WAN Connector set up as a DHCP server, and connecting to the Internet.
  a(Magic WAN Connector)--> b(Internet) --> c(Cloudflare)

  subgraph Customer site
  d[LAN 1] --> a
  e[LAN 2] --> a
  end

  classDef orange fill:#f48120,color: black
  class a,c orange
```

In the example below, the Magic WAN Connector device sits behind the WAN router in your site, and on-ramps only some of the existing LANs to Cloudflare.

```mermaid
flowchart LR
	accTitle: Magic WAN Connector connects to the router in the site, and only some of the LANs connect to Connector.
  a(Magic WAN Connector)--> b((Site's router)) --> c(Internet) --> i(Cloudflare)

  subgraph Customer site
  d[LAN 1] --> a
  e[LAN 2] --> a
  g(LAN 3) --> b
  h(LAN 4) --> b
  end

  classDef orange fill:#f48120,color: black
  class a,i orange
```

Refer to [Magic WAN Connector deployment options](https://developers.cloudflare.com/reference-architecture/diagrams/sase/magic-wan-connector-deployment/) for a high-level explanation of the deployment options that make sense to most environments, as well as a few advanced use cases.

#### Firewall settings required

If there is a firewall deployed upstream of Magic WAN Connector, configure the firewall to allow the following traffic:

| Protocol/port | Destination IP/URL | Purpose |
| - | - | - |
| `UDP/53` | DNS destination IP `1.1.1.1` | Needed to allow DNS traffic to Cloudflare DNS servers. Cloudflare uses this port for DNS lookups of control plane API. |
| `TCP/443` | - | Magic WAN Connector will open outbound HTTPS connections over this port for control plane operations. |
| `UDP/4500` | Destination IP `162.159.64.1` | Needed for Magic WAN Connector initialization and discovery through outbound connections. |
| `UDP/4500` | Destination IP - Cloudflare anycast IPs | Needed for the Cloudflare anycast IPs assigned to your account for tunnel outbound connections. This traffic is tunnel traffic. |
| `TCP/7844`, `UDP/7844` | Outbound connections | Used to support debugging features in Magic WAN Connector. |
| `UDP/123` | `http://time.cloudflare.com/` | Needed for Magic WAN Connector to periodically contact Cloudflare's Time Services. |

## Activate appliance

The Magic WAN Connector is shipped to you deactivated, and will only establish a connection to the Cloudflare network when it is activated. Cloudflare recommends leaving it deactivated until you finish [setting it up in the dashboard](#set-up-cloudflare-dashboard).

When Magic WAN Connector is first activated, you need to have Internet connection. If you chose to set up your Magic WAN Connector with DHCP you will need to have one of the Magic WAN Connector ports connected to the Internet through a device that supports DHCP. This is required so that the Magic WAN Connector can reach the Cloudflare global network and download the required configurations that you [set up](#set-up-cloudflare-dashboard).

If you set up your Magic WAN Connector with a static IP through the bootstrap method, you do not need a DHCP port. Refer to [DHCP vs static IP connections](#decide-on-dhcp-vs-static-ip-connections) for more information.

Warning

Remember that if you chose the DHCP method you have to connect Magic WAN Connector through a route that supports DHCP for its first connection to the Internet. Otherwise, Magic WAN Connector will not work.

When you are ready to connect your Magic WAN Connector to the Cloudflare network:

1. In the Cloudflare dashboard, go to Magic WAN's **Configuration** page.

[Go to **Configuration**](https://dash.cloudflare.com/?to=/:account/magic-wan/configuration)

1. Go to **Connectors**.
2. Find the Magic WAN Connector you want to activate, select the three dots next to it > **Edit**. Make sure you verify the serial number to choose the right Magic WAN Connector you want to activate.
3. In the new window, the **Status** dropdown will show as **Deactivated**. Select it to change the status to **Activated**.
4. The **Interrupt window** is the time period when the Magic WAN Connector software can update, which may result in interruption to existing connections. Choose a time period to minimize disruption to your sites. Refer to [Interrupt window](https://developers.cloudflare.com/magic-wan/configuration/connector/maintenance/interrupt-service-window/) for more details on how to define when the Magic WAN Connector can update its systems.
5. Select **Update**.

***

## WAN with a static IP address

After activating your device, you can use it in a network configuration with the WAN interface set to a static IP address — that is, an Internet configuration that is not automatically set by DHCP. To use your Magic WAN Connector on a network configuration with a static IP, follow the steps below.

Warning

Make sure you complete the setup workflow and activate your Magic WAN Connector before changing the WAN settings to a static IP.

1. Connect Magic WAN Connector to a DHCP port with access to the Internet.
2. [Add a Connector on-ramp](#add-a-connector-on-ramp) in the Cloudflare dashboard.
3. Create a [DHCP WAN](#create-a-wan).
4. [Activate](#activate-appliance) and power on your Magic WAN Connector.
5. Wait 60 seconds.
6. Make changes to the [WAN settings](#create-a-wan) in the Cloudflare dashboard to a static IP set up.
7. Wait 60 seconds again.
8. Magic WAN Connector will go offline. This is normal and expected behavior.
9. Adjust your physical connections as required to match the static configuration.
10. Magic WAN Connector comes back online.

## Bootstrap via Serial Console

Advanced users can locally configure their Magic WAN Connector to work in a static IP configuration. This local method does not require having access to a DHCP Internet connection. However, it does require being comfortable with using tools to access the serial port on Magic WAN Connector as well as using a serial terminal client to access the environment in your Magic WAN Connector.

Below is a detailed description of how to use the serial port to configure your Magic WAN Connector locally.

Note

The `reset device` option in your Magic WAN Connector clears most of the configuration that is locally cached, resets the password to the default, and reboots.

### Equipment required

To access the serial port on Magic WAN Connector you will need the following equipment:

* The Magic WAN Connector device
* A Phillips-head screwdriver
* A micro-USB to USB-A cable (there should be one included in the packaging of your Magic WAN Connector device)
* A computer with an available USB port
* A serial terminal client
* Optional: if needed, a USB-A to USB-C converter dongle if your computer requires it

### 1. Access the device's serial port

1. Using the Phillips screwdriver, loosen the screw covering the serial console panel on the back of the Magic WAN Connector and turn the panel out of the way.
   * Pictures and more instructions can be found on [Dell's Technical Documents](https://www.dell.com/support/kbdoc/en-us/000134440/how-to-access-console-port-of-dell-emc-networking-virtual-edge-platform-1405-series).
2. Connect your computer to your Magic WAN Connector device using the USB cable.

#### Default password

The default password for your Magic WAN Connector device is the serial number (also known as a Service Tag for Dell devices), all uppercase followed by an `!` (for example, `A1B2C3D!`)

### 2. Install a serial terminal client

To access the Magic WAN Connector device environment you need a serial terminal client. Follow the instructions below to install one, based on your operating system.

#### Windows

Cloudflare recommends using PuTTY for Windows. Download PuTTY from the [official website](https://www.putty.org/) and then install it.

1. Check the COM port of the USB to UART device in the Windows Device Manager. It should show up as something similar to `Silicon Labs CP210x USB to UART Bridge (COMX)`.
2. Take note of the value in the parentheses (COMX).
   * Refer to the [Dell Documentation Page](https://infohub.delltechnologies.com/l/virtual-edge-platform-vep-1405-series-diag-os-and-tools-release-notes/bios-installation-and-configuration) for more details on creating a serial console connection.
3. Launch PuTTY.
4. Under **Category**, make sure that **Session** (the first item) is selected.
5. Under **Connection type**, select **Serial**.
6. In the **Serial Line**, type in the COM port found in step 2 (for example, `COM1`).
7. In the **Speed**, enter `115200`.
8. Select Open on the bottom of the dialog box. A terminal window should pop up.
9. The screen may need to be manually refreshed when a new device is connected. You can do that by pressing `CTRL + C`.

#### macOS

Cloudflare recommends installing Screen for macOS. You can install Screen via `brew install screen`. If you do not have `brew` installed, follow the instructions on [Brew's Official Website](https://brew.sh/) to install it.

1. Open the macOS Terminal.
2. Run `ls /dev/cu.*` to list the connected serial devices.
3. The command should return an output similar to `/dev/cu.usbserial-0001`. Copy this output to the clipboard or note this down somewhere else.
4. Run `sudo screen -adRUS mconn <PATH_FROM_STEP_3> 115200`.
5. The screen may need to be manually refreshed when a new device is connected. You can do that by pressing `CMD + C`.

#### Linux

Cloudflare recommends installing Screen for Linux. You can install Screen via your package manager of choice. For example, for Debian/Ubuntu, install by running `sudo apt update && sudo apt install screen`

1. Open Terminal.
2. List the connected serial devices by running `ls /dev/serial/by-id/*`.
3. The command should return an output similar to `/dev/serial/by-id/usb-Silicon_Labs_CP2102_USB_to_UART_Bridge_Controller_0001-if00-port0`. Copy this to the clipboard or note this down.
4. Run `sudo screen -adRUS mconn <PATH_FROM_STEP_3> 115200`.
5. The screen may need to be manually refreshed when a new device is connected. You can do that by pressing `CTRL + C`.

### 3. Configure a static IP

The `reset device` option in your Magic WAN Connector clears most of the configuration that is locally cached, resets the password to the default, and reboots.

1. Log into your Magic WAN Connector device. You will be prompted to change your password if you attempt to log in with the default password.
2. From the menu, go to **Bootstrap** with the arrow keys and select it with the Enter key.
3. Select the jack (physical port) you want to configure for the initialization of the connector.
4. Enter the VLAN tag (if applicable) of the network. Leave it blank if untagged.
5. Select the `static` option as your network type.

Note

The main reason to use the bootstrapper is if every network your Magic WAN Connector device is plugged into is either static, behind a VLAN, or both. If you find yourself here and configuring a network with DHCP and no VLAN, you are probably not in the right place. See the section on configuring your Magic WAN Connector [via the dashboard](#set-up-cloudflare-dashboard).

1. Enter the IP address you would like the connector to have in CIDR form (for example, `10.0.0.2/24`).
2. Enter the IP address of the Internet gateway (this must be in the same subnet as the previous IP address you entered and must not be the same address).
3. Select **Save** and confirm that you want to use the new settings.
4. The Magic WAN Connector will download the rest of the settings from Cloudflare. The last heartbeat of the Magic WAN Connector should update once it has made contact with Cloudflare.

***

## About high availability configurations

You need to deploy two Connectors in your premises before you can set up a site in high availability. When you set up a site in high availability, the WANs and LANs in your Magic WAN Connector have the same configuration but are replicated on two nodes. In case of failure of one of the devices, the other device becomes the active node, taking over the configuration of the LAN gateway IP and allowing traffic to continue without disruption.

Because Magic WAN Connectors in high availability configurations share a single site, you need to set up:

* **Static address**: The IP for the primary node in your site.
* **Secondary static address**: The IP for the secondary node in your site.
* **Virtual static address**: The IP that the LAN south of the Magic WAN Connector device will forward traffic to, which is the LAN's gateway IP.

Make sure all IPs are part of the same subnet.

For detailed information about the expected behavior of high availability configurations, refer to the [High availability configurations](https://developers.cloudflare.com/magic-wan/configuration/connector/reference/#high-availability-configurations) reference page.

### Create a high availability configuration

You cannot enable high availability for an existing site. To add high availability to an existing site in the Cloudflare dashboard, you need to delete the site and start again.

To set up a high availability configuration:

1. Follow the steps in [Add a Connector on-ramp](#add-a-connector-on-ramp) up until step 4.

1) After naming your site, select **Turn on high availability**.
2) Select **Create and continue**.
3) Select **Add Connector**.
4) From the list, choose your first Magic WAN Connector > **Add Connector**.
5) Back on the previous screen, select **Add secondary Connector**.
6) From the list, choose your second Magic WAN Connector > **Add Connector**.
7) Select **Continue** to create a WAN. If you are configuring a static IP, configure the IP for the primary node as the static address, and the IP for the secondary node as the secondary static address.
8) To create a LAN, follow the steps mentioned above in [Create a LAN](#create-a-lan) up until step 4.
9) In **Static address**, enter the IP for the primary node in your site. For example, `192.168.10.1/24`.
10) In **Secondary static address**, enter the IP for the secondary node in your site. For example, `192.168.10.2/24`.
11) In **Virtual static address**, enter the IP that the LAN south of the Magic WAN Connector device will forward traffic to. For example, `192.168.10.3/24`.
12) Select **Save**.
13) From the **High availability probing link** drop-down menu, select the port that should be used to monitor the node's health. Cloudflare recommends you choose a reliable interface as the HA probing link. The primary and secondary node's probing link should be connected over a switch, and cannot be a direct connection.
14) Follow the instructions in [Set up your Magic WAN Connector](#set-up-your-magic-wan-connector) and [Activate appliance](#activate-appliance) to finish setting up your Connectors.

***

## IPsec tunnels and static routes

Magic WAN Connector automatically creates [IPsec tunnels](https://developers.cloudflare.com/magic-wan/reference/gre-ipsec-tunnels/#ipsec-tunnels) and [static routes](https://developers.cloudflare.com/magic-wan/reference/traffic-steering/) for you. You cannot configure these manually.

To check the IPsec tunnels and static routes created by your Magic WAN Connector:

1. In the Cloudflare dashboard, go to the **Sites** page.

[Go to **Sites**](https://dash.cloudflare.com/?to=/:account/magic-wan/sites)

1. Select the name of the site for which you want to check the Magic WAN Connector's IPsec tunnels and static routes, and select **Edit**.
2. Select **Tunnels** to check IPsec tunnels, and **Routes** for the static routes.

***

## Next steps

* [Network options](https://developers.cloudflare.com/magic-wan/configuration/connector/network-options/)
* [Maintenance](https://developers.cloudflare.com/magic-wan/configuration/connector/maintenance/)
* [Reference information](https://developers.cloudflare.com/magic-wan/configuration/connector/reference/)
* [Troubleshooting](https://developers.cloudflare.com/magic-wan/configuration/connector/troubleshooting/)
